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Drinking Fountains:
The Drinking Fountain in the Playground needs to be turned off and the lines drained for winter. We recommend turning it off before November 10th and leaving it off until all danger of freezing conditions has past, usually by early April. If it does freeze with water in it, it will break the Drinking Fountain. Your Drinking fountain is most likely the Most Dependable Fountains model # 10145 SMSS. Most Dependable Fountains, Inc. can be contacted at 901-867-0039 or www.mostdependable.com/contact/to order additional parts.

Color Seal (Art on the Ground and Painted Courts):
Color Seal can last several years if treated properly. The greatest damage to Color Seal is done accidentally during snow removal. Please observe the following to best protect the surface:
· Do not use chains on tires on the color seal area.
· When it is necessary to use a plow, cover the sharp edge with a cloth or rag to prevent scraping of the color seal.
· Avoid excessive salt use (Please note excessive salt use can also damage concrete curbs); NYC DPR recommends sand or calcium chloride not rock salt

Trees and Plantings:
Trees need the most care during the first two years of their planting in the Playground. Fill the “Gator” bags at least once a week during the warm months, and twice a week during the heat of summer or during drought conditions. Plantings on the playground should also be watered on the same schedule. Once they make it past two years they have a great chance of making it to 80 years! After one year the tree stakes and tree ties should be removed. If you are experiencing difficulty with weeds or tree care please reach out to us at Tiffany.Briery@TPL.org so we can help!

Turf Fields:
Turf fields cannot be plowed, snow must be allowed to melt on them. If seams are spreading or ripping shortly after installation IMMEDIATELY contact the turf manufacturer. Dealing with turf issues in a timely manner prevents more damage.
Leaf blowers can be used on Turf Field, but exercise caution not to disturb the infill, if your field has rubber or sand infill.

Play equipment / repairs / maintenance
· GameTime  contact:  JoAnn Thomas jthomas@mrcrec.com    800-922-0070 Ext. 1011
· Kompan contact:   Ken Dobyns  KenDob@Kompan.com 646-596-1052
· Maintenance: check bolts, hand holds on play equipment annually 
· Graffiti removal specs are in the Stewardship Manual Appendix 
· Copy the Trust for Public Land on any correspondence with play equipment manufacturers so we can keep up on any issues. Tiffany.Briery@tpl.org

Thank you for all your dedication and hard work in keeping the playgrounds beautiful!
